
**KQ 380 Actual Cooktop w/o Beveled Edge (1.5” for Bevel)**

Height of the warming shelf from the cooktop – 13.75”

Measuring underneath the warming shelf on the cooktop – 6.75”

Warming shelf top – 6.5”



Leg Height – 9.5”

Leg to Leg Depth – 19.5”

Body Depth – 20”

Leg to Leg Width – 35”

Body Width – 36.5”

Overall Stove Height (to the top of the warming shelf) – 51.25”

Floor to Cooktop – 32”


Back of Flue to center – 3.75”

**KQ 480 Actual Cooktop w/o Beveled Edge (1.5” for Bevel)**

Height of the warming shelf from the cooktop – 14.75”

Measuring underneath the warming shelf on the cooktop – 8.75”

Warming shelf top – 8.5”



Leg Height – 10”

Leg to Leg Depth – 21.75”

Body Depth – 22.75”

Leg to Leg Width – 43”

Body Width – 45.5”

Overall Stove Height (to the top of the warming shelf) – 55”

Floor to Cooktop – 34.5”

Back of Flue to center – 4”